Zeiss Ikon Box Tengor N, BII, D
This is a Google translate of the German booklet.
D- Slider in which the aperture openings are located condition
F1, F2 - Springs on which the pins Z1and Z2 are located
L - Lever to release the shutter
R - Device for locking the two camera halves
S - Key for winding the roll of film on the empty spool
T - Slider to adjust the shutter for time recordings
V - Opening for screwing in the wire release
W1 - Viewfinder for high shots
W2 - Viewfinder for landscape shots
X - Slider with group and portrait attachment lens
Z1, Z2 - Fasten pins on springs F1 and F2 holding the coil
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Figure 3 - Box tengor disassembled
Loading the cameras

Applies to the 6×9 and 6.5×11 cm apparatuses

Pull out latch R (Figure 1),

whereupon the camera splits into two

Disassemble in half left (Figure 3).

Pull out latch R (Figure 1),

whereupon the camera splits into two

Disassemble in half shells (Figure 3).

The coil is at both ends hollow to allow the  peg to

be plugged into the bobbin bearings

can.  One end is slit (Figure 2), the other has a circular

opening.
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Fig.4 Inserting the empty spool

The coil with the right hand on the jaw of the slotted end, on pin 22  (fig. 3).

Press spring F2 sideways and

the slotted end of the coil on the key

drive past and put on the inner lock pivot
Then turn the key until it engages the coil and carries it with it.
Insert the full spool so that the tip of the protective paper is on top and after the sliding roller is directed. The spool will fit the Pin Z1 set, spring F1 pushed aside.
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Fig. 5 Inserting the full spool and the other end of the coil on the fixed pivot brought by until this in the round coil opening occurs.  Release paper fasteners, protective tape over the two rolls on the image section of the camera drove past and the tip into the longer slot

insert the empty bobbin.

Then the key turn a few times in the direction of the arrow, to hold stripes. Then put the two halves back together.
Figure 6 Attaching the end of the film to the empty spool.
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The shutter
Snapshots are created by pressure on lever L (Fig. 7).

Pull out slider T for time recordings.

Pressing lever L opens the shutter.

As soon as the pressure stops, it closes. (Time exposure)
The release of the shutter can also be done with the help of a cable release, which is the opening 7 is screwed.
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Fig. 7 Ancillary lenses and diaphragms
close-up lenses:
A slider X is built into both models,

in which there are two supplementary lenses:

:one for group shots, distance 4 meters

: one for close-ups, distance 1 meter

Condition. When you pull out the slider, appears

first the sign <Gr4> for the group lens,

then <portr. 1> for the portrait lens.

The correct position is at a distinct snapping evident
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Fig. 8 Further removal of the exposed film.
Bezels
In slide D there are 3 openings, F 11, F 18 and F25, each of which changes when moving by snapping in a spring-loaded locking lever makes known.  The smaller the opening, the the image becomes sharper; the larger the opening is,

the shorter the exposure must be."
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Removing the exposed film

Protective paper through after the last exposure Turn the film key, roll it up all the way, camera Open and as described on page 3 Spool with the sticky paper attached to the end close.
When removing the film, to the side

of the springy film carrier towards the other end

hold the spool lightly to prevent it from being flung out

(Fig. 8).
Also remove the empty spool and put it in the <key camp>  (top slot) deploys so that the apparatus ready to record pictures.


BOX – TENGOR  5 - 7.5 cm
Setting up and handling the box -Tengor

5x7.5 cm generally agree with those of

other formats. Only in the following

Points - there are small differences:
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Figure 9 – Box Tengor 5 x 7.5cm
1. The film spool has one on one side

pin, with which they fit into the spring bearing of the

spool holder on the opposite side of the film key

side is used.
2. The Camera 5x7.5cm is with a fixed aperture of F:11
3. A group auxiliary lens containing Slider X is not on the 5-7.5 cm model required because of the focus area of ​​the lens from infinity to about 3 m away suffices.
A Portrait conversion lens can be used.

Can be supplied on request against calculation. (the close up lens will state distance from lens required)
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1. The film spool has one on one side pin, with which they fit into the spring bearing of the spool holder on the opposite side of the film key overlying side is used.
2. The camera is 5×7.5 cm with a fixed Aperture F:11 fitted.  
3. A group auxiliary lens containing Slider X is not on the 5×7.5 cm model

required because of the focus area of ​​the lens

from infinity to about 3 m away suffices.
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GENERAL REMARKS
Treatment of the camera
One first tries all the movements which the

'Instructions for use indicates before loading the

Camera”. Since the camera is not a worthless game

. should be zelrg, one must treat them lovingly,

do not expose to the rain or into the wet grass

place, but in the leather case that is also available

keep protected. (Be nice to your expensive camera)

All applied

Care is for the film, not the lens ultimately of great advantage for the picture.


Recording material
Everywhere you ask for the matching Zeiss roll film
(N for 5x.7.5, BII for 6x9, D for 6.5x11 cm), which with proper treatment pro-delivers daily results.  The film spools are lightproof when closed. you let therefore use the camera in daylight and after full exposure as well take out daylight.  But that's not it

said to expose the coil to bright light

should. Keep them in a dark

Places (in a closet or the like.) At medium

Temperature up and set it even with something steamed light into the camera.
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Recording
a) Snapshots

(The shutter speed corresponds to 1 exposure time of approx. 11 of a second).  (Remember film was slow then, like 10 ASA)  Snapshots are only taken in sunshine made, i.e. the object to be recorded must be in sunlight, but must not shine into the lens.
man points the camera at the object to be photographed and convinces himself of it; that also the whole 

subject to be photographed appears in the viewfinder.  If the apparatus is correctly adjusted to the picture,

so you move the locking lever carefully,

without shaking the camera, after the other

side of the shield. You hold the camera

firmly against the body and make sure

that they are held horizontally, i.e. not pointing upwards or downwards, because otherwise directory '

occur. Immediately after the recording you turn the 
key until the next section of the film is in the recording position.

b) time recordings
So the picture doesn't change (blur) ready on a solid base (tripod, table, pole or the like.) rest while you are careful most expedient

you work with the cable release.

For attachment to the tripod has the

Camera tripod nuts for portrait and landscape photography.

After completing the time recording

the apparatus again and again for a snapshot

a, i.e. H. you push the two sliders D

and T all the way back in.
c) recruitment
At full aperture, the lens captures all objects

lying between 4 m and infinity are sharp

again. For most recordings, rnan

so at the distance of the object none

to take into account. For distances below

4 m come the ones mentioned on page 7

Additional lenses to consider
At full aperture, the lens captures all objects

lying between 4 m and infinity are sharp

again. For most recordings you need

so at the distance of the object none

to take into account. For distances below

4 m come the ones mentioned on page 7

Additional lenses to consider
d) exposure time
Generally, one gets outdoors with snapshots

get by with unfavorable lighting conditions. However, if you are forced also to take outdoor time shots, both

in landscape photography as well as group and portrait shots.  The necessary exposures are taken expediently

the Zeiss Ikon exposure board, which is possible for everyone.

For information about the most suitable exposure time

gives.
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When recording people in the room

you will always use the widest aperture to

get by with exposures that are as short as possible. (You are still doing time exposures)
The exposure time is irrelevant here

only according to the intensity of the outside light, but

also depends on the brightness of the room

(Size and number of windows, color of the wallpaper

etc.). Again, the exposure board is on good guide to the right exposure time.
